{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":6,"n_cols":15,"rows_kept":6,"merged":[[0,0,0,14],[2,10,5,10],[2,11,5,11],[2,12,5,12],[2,13,5,13]],"flags":["formulas_cached_only"]}
["甘煤一公司（矿二红沙梁项目部）2026年1月下旬所需物资（一标段）明细表"]
["物资编号","分类编码","物料分类","物资名称","规格型号","单位","数量","税率","技术要求及执行标准","品牌/厂家","进货日期","标段划分","付款形式及周期","使用单位","备注"]
[1,null,null,"托架\n（加工件）","厚度20mm","套",256,{"v":0.13,"d":"13%"},"料材：Q235-A     防腐采用《煤矿井筒装备防腐蚀技术规范》（MT/T 5017-2011)“表A.3 重防腐涂层体系及最小涂层厚度”","/","中标后5日内送达","一标段","挂账后3个月内付清","甘肃煤炭第一工程有限责任公司矿建第二分公司红沙梁矿建项目部","防腐标准：构件涂装前进行预处理，预处理采用喷砂除锈方式，除锈等级应达到Sa3级。预处理后涂刷环氧富锌底漆1～2道，涂刷环氧沥青类防护面漆，至少3道。漆膜总厚度不小于200μm，漆膜附着力用划格法测试不应低于85%。加工件详见附图     含运费"]
[2,22050001,null,"工字钢","25b","米",640,{"v":0.13,"d":"13%"},"料材：Q345 防腐采用《煤矿井筒装备防腐蚀技术规范》（MT/T 5017-2011)“表A.3 重防腐涂层体系及最小涂层厚度”","/",{"$nulls":4},"10M/根   含运费"]
[3,null,null,"托管大梁\n（加工件）","长度：6300mm","根",6,{"v":0.13,"d":"13%"},"料材：Q345 防腐采用《煤矿井筒装备防腐蚀技术规范》（MT/T 5017-2011)“表A.3 重防腐涂层体系及最小涂层厚度”","/",{"$nulls":4},"加工详见托管大梁图  \n含运费"]
[4,16060015,null,"U型螺栓","M18","套",256,{"v":0.13,"d":"13%"},"料材：Q235-A  镀锌防腐","/",{"$nulls":4},"加工件详见U型螺栓加工图配套2倍的螺母及平垫弹垫。 含运费"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}