{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"images":5},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":67,"n_cols":6,"rows_kept":67,"flags":["formulas_cached_only"]}
["序号","物料名称","规格型号","单位","数量","备注"]
[1,"耐磨三通","DN300,图号0468-01000-04236-16-025详见附图（山东丁壬机电设备有限公司/江苏冠诚冶金设备有限公司）\n180-SPT-4301，耐磨层为整体式，底部耐磨层在原有基础上增加半球形","件",2,"气化装置耐磨件"]
[2,"耐磨三通","DN350,图号0468-01000-04236-16-0275180-SPT-4402，详见附图（山东丁壬机电设备有限公司/江苏冠诚冶金设备有限公司）耐磨层为整体式，底部耐磨层在原有基础上增加半球形","件",1,"气化装置耐磨件"]
[3,"耐磨三通","DN400,图号0468-01000-04236-16-0265180-SPT-4401，详见附图（山东丁壬机电设备有限公司/江苏冠诚冶金设备有限公司）耐磨层为整体式，底部耐磨层在原有基础上增加半球形","件",1,"气化装置耐磨件"]
[4,"耐磨三通","DN600,图号0468-01000-04236-16-0285180-SPT-4601，详见附图（山东丁壬机电设备有限公司/江苏冠诚冶金设备有限公司）耐磨层为整体式，底部耐磨层在原有基础上增加半球形","件",2,"气化装置耐磨件"]
[5,"耐磨三通","DN750,图号0468-01000-04236-16-0295180-SPT-4801，详见附图（山东丁壬机电设备有限公司/江苏冠诚冶金设备有限公司）耐磨层为整体式，底部耐磨层在原有基础上增加半球形","件",2,"气化装置耐磨件"]
[6,"浮动套","470*282*50mm，详见附图","个",2]
[7,"耐磨球阀","DN100  class150 碳钢 内衬耐磨层 介质:气化黑水","台",2,"气化装置耐磨件"]
[8,"同心耐磨异径","DN100x50 外壁20#钢 内衬耐磨层 介质:气化黑水","个",3,"气化装置耐磨件"]
[9,"异径耐磨三通","DN100x50 外壁20#钢 内衬耐磨层 介质:气化黑水","个",3,"气化装置耐磨件"]
[10,"等径耐磨三通","DN125x125 外壁20#钢 内衬耐磨层 介质:气化黑水","个",2,"气化装置耐磨件"]
[11,"同心耐磨异径","DN65x50 外壁20#钢 内衬耐磨层 介质:气化黑水","个",3,"气化装置耐磨件"]
[12,"耐磨截止阀","DN100  class150 碳钢 内衬耐磨层 介质:气化黑水","台",2,"气化装置耐磨件"]
[13,"带颈法兰","DN100 SH/T3406 SO-RF Class150","个",4]
[14,"防溢裙板","TIPTOP,长度15米","条",4]
[15,"防溢裙板","TIPTOP,长度12米","条",2]
[16,"防溢裙板","TIPTOP,长度10.5米","条",4]
[17,"防溢裙板","TIPTOP,长度22.5米","条",4]
[18,"电动葫芦钢丝绳","直径：11mm，结构形式：D-6*37+1","米",35]
[19,"电动葫芦钢丝绳","直径：11mm-6*37M-FC-1770","米",46]
[20,"筛板","厚40mm，材质：聚氨酯","件",5,"捞渣机振动脱水筛（青岛正大电力环保设备有限公司）"]
[21,"不锈钢滤网","80目，304，配套过滤器GL41H-150LBC DN250使用，每只滤网配套端盖金属缠绕垫4片。","个",3,"温州东斯特阀门管件制造有限公司"]
[22,"不锈钢外丝宝塔球阀","3分外丝/8mm宝塔（材质316）","个",10]
[23,"碳钢管","外径457mm，厚度22mm,材质：碳钢","米",{"v":9.5,"d":"10"}]
[24,"缠绕垫","RF Class600 THK=4.5mm D1221 SH/3407","片",3]
[25,"八角垫","DN200-1500 材质：316L","个",1]
[26,"自洁式空气过滤器滤芯","外径：Ф320mm内径：Ф220mm高度：1000mm内/外支撑网：镀锌 上/下盖材质：ABS 滤料材料：复合纤维密封圈材质：聚氨酯\n过滤等级：EN779-2012  数值：F7额定风量：EN779-2012 1320m3/h有效过滤面积：28m3","个",420]
[27,"不锈钢耐震压力表","Y-100  0-1Mpa  精度等级1.6 螺纹316L","块",4]
[28,"不锈钢耐震压力表","Y-100  0-10Mpa  精度等级1.6 螺纹316L","块",6]
[29,"不锈钢耐震压力表","Y-100  0-60Kpa  精度等级1.6 螺纹316L","块",1]
[30,"旋启式止回阀","DN100  CL150 法兰面：RF\n材质：H2A1A05-G3 20#钢\n阀门长度：292mm 用于低压蒸汽包补水止回阀","台",1]
[31,"Y型截止阀","DN20 CL300  法兰面：RF材质：316L\n阀门长度：178mm用于中压甲铵冷凝器排放管导","台",1]
[32,"截止阀","DN15 CL150  法兰面：RF材质：304L\n阀门长度：108mm ","台",1]
[33,"Y型截止阀","DN20 CL150  法兰面：RF\n材质：316L\n阀门长度：117mm","台",1]
[34,"O型密封圈","70.3*3.1，三元乙丙 GB/T3452-2007","个",100]
[35,"万向轮骨架密封","型号：SW-32-01 RF尺寸：DF80*50*11.5 材质：RF+A500 液氨装车鹤管使用","件",8]
[36,"液氨液相鹤管快速接头附带紧急拉断阀","法兰连接及标准: HG/T20615-2009 CL300 WN/RF DN50/50\n 鹤管管道口径DN50 鹤管液相附带DN50插焊连接螺栓致断拉断阀PN40-S30408   接车方式：液相DN50(快速接头）-S30408 法兰执行：HG/T20615-2009","套",1]
[37,"承插焊闸阀","DN20 800LB Z3A6A03-P2G3","个",10]
[38,"承插焊闸阀","DN25 800LB Z3A6A03-P2G3","个",10]
[39,"圆盘式蒸汽疏水阀","型号：HRF150A CL2500 尺寸：DN25 RJ 材质：F22 CL3/WC9  最高工作压力：15MPa,最低工作压力：1.6MPa,正常工作温度压力：11.7MPa/566℃ 法兰执行：HG/T20615-2009","个",3]
[40,"浮球式疏水阀","DN20 SC41H-150LB RF  法兰执行：HG/T20615-2009","个",5]
[41,"浮球式疏水阀","DN25 SC41H-150LB RF 法兰执行：HG/T20615-2009","个",5]
[42,"防尘网","绿色 四针 8m*30m","卷",60]
[43,"单头螺栓/螺母","M8*16 ，材质：316L，带弹垫GB/T5783","套",100]
[44,"单头螺栓/螺母","M10*16，材质：316L，带弹垫GB/T5783","套",50]
[45,"PE管","DN15，PN10，热熔GB/T13663-2018","根",3]
[46,"PE管","DN20，PN10，热熔GB/T13663-2018","根",3]
[47,"PE管","DN25，PN10，热熔GB/T13663-2018","根",3]
[48,"PE双由令球阀","DN15","个",5]
[49,"PE双由令球阀","DN20","个",5]
[50,"PE双由令球阀","DN25","个",5]
[51,"PE直接","DN15 PN10","个",5]
[52,"PE直接","DN20 PN10","个",5]
[53,"PE直接","DN25 PN10","个",5]
[54,"PE弯头","DN15 PN10 90°","个",5]
[55,"PE弯头","DN20 PN10 90°","个",5]
[56,"PE弯头","DN25 PN10 90°","个",5]
[57,"UPVC管","De20 PN1.0（国标，化工级）","根",2]
[58,"UPVC管","De25 PN1.0（国标，化工级）","根",2]
[59,"UPVC管","De32 PN1.0（国标，化工级）","根",2]
[60,"UPVC直接","DN15 PN1.0（国标，化工级）","个",5]
[61,"UPVC直接","DN20 PN1.0（国标，化工级）","个",5]
[62,"UPVC直接","DN25 PN1.0（国标，化工级）","个",5]
[63,"UPVC弯头","DN15 PN1.0（国标，化工级） 90°","个",5]
[64,"UPVC弯头","DN20 PN1.0（国标，化工级） 90°","个",5]
[65,"UPVC弯头","DN25 PN1.0（国标，化工级） 90°","个",5]
[66,"卡扣抱箍","Ø325管道使用","件",10]